PRPLC-S01-XXX-XXX
Planar light wave circuit splitter, insert type
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· Small size, high reliability, wide operating wavelength range                                              
· Application for EPON, GPON, FTTx networks
· G657A1 fiber or customer specified  
· [bookmark: _Hlk101524996]Splitter ration from 1:2 to 1:64                                           

Part number

	PRPLC-S01-XXX-XXX
	Planar light wave circuit splitter, insert type

	            1   2

	*1 indicate splitter capacity:102=1X2;202=2X2;104=1X4;204=2X4;108=1X8;208=2X8;116=1X16;216=2X16…

	*2 indicate the splitter adapter style: FC=FC; FCA=FC/APC; LC=LC; LCA=LC/APC; SC=SC; SCA=SC/APC…

	


Performance

	Parameters
	Specification

	Operating wavelength (nm)
	1260-1650

	Type
	1X2
	1X4
	1X8
	1X16
	1X32
	1X64

	Insertion loss (dB)
	≤3.8
	≤7.1
	≤10.2
	≤13.3
	≤16.5
	≤19.8

	Loss uniformity (dB)
	≤0.3
	≤0.3
	≤0.3
	≤0.5
	≤0.5
	≤1.0

	PDL (dB)
	≤0.08
	≤0.08
	≤0.08
	≤0.1
	≤0.1
	≤0.2

	Type
	2X2
	2X4
	2X8
	2X16
	2X32
	2X64

	Insertion loss (dB)
	≤3.8
	≤7.1
	≤10.2
	≤13.3
	≤16.5
	≤20.1

	Loss uniformity (dB)
	≤0.5
	≤0.5
	≤0.5
	≤0.8
	≤0.8
	≤1.5

	PDL (dB)
	≤0.1
	≤0.1
	≤0.1
	≤0.15
	≤0.15
	≤0.3

	Return loss (dB)
	≥55

	Directivity (dB)
	≥55

	Wavelength dependent Loss (dB)
	≤1.0

	Pigtail length (m)
	1.0m or customer specified

	Fiber type
	ITU G657A1 or customer specified

	Operating temperature (℃)
	-40℃ to +85℃

	Storage Temperature (℃)
	-40℃ to +85℃









While the information has been carefully compiled to the best of our knowledge, nothing is intended as representation or warranty on our part and no statement herein shall be construed as recommendation to infringe existing patents. In the effort to improve our products, we reserve the right to make changes judged to be necessary.
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